Caterham Superlight R 1999

Fuse label strip, print on sticker sheet and adhere to relay stack.

Overall height 157mm

Width 32mm

|  |
| --- |
| Fuel Pump 15A  ECU (Inj. Only) 20A |
| Brake/Reverse Light 15A  Instruments/Heater 10A  Radiator Fan 15A |
| Heated Screen 10A  Rear Fog Light 5A  R/H Side Tail Light 7.5A |
| L/H Side Tail Light 5A  Main Beam 15A  Dip Beam 15A |
| Wipe/Wash 15A  Horn 20A  Flasher Unit 10A |